**Firmware upgrade**

Step 1: Open the host computer, click Update on the right, enter the password 123, and enter the firmware upgrade interface. As shown in Figure 1:




Figure 1

Step 2：Search for the battery, select the battery, open the folder, select the program, and click Download. As shown in Figure 2：




Figure 2

Step 3: On the host computer interface, click Config to enter the system configuration interface, the CAN protocol needs to be set to the Victron protocol, modify the FullChgTotalVolt parameter to 52.5V, and click Write. As shown in Figure 3：




Figure 3